**Mitre trimmer**

* Handle can be set vertical using locking bolt at rear – sign required?
* Wooden guard to protect exposed blade
* Sign to say ‘keep fingers out’ underneath

**Disc sander**

* Cleaning discs – resin or wire brush

**Scroll saw**

* Wing nut for guard to replace existing nut?
* See if we can locate a manual

**All power tools set on bench**

* Mark the cables/plugs so we know which is which

**Pillar drill**

* Sign to say ‘goggles must be worn’ – as no guard
* Note to say how to change speed
* Floor level isolator
* Sharpening station (LIDL or similar) for bits

**Planer thicknesser**

* Blade tool setter – (jig online search throws up several are they right?)
* Metal polish on each of the beds
* Warning – no hands ahead of the exit roller
* Status of replacement belt?
* Floor level isolator?

**Bandsaw**

* Bearing adjustment required – too much blade ‘play’
* Vacuum wheels inside top and bottom

**Router table**

* Set of router cutters?
* Diamond pen file?

**Morticer**

* Set up incorrectly – changed
* Augur needs to reach both retainers
* 7/16 spanner required when changing
* Imperial Allen key required
* Buy small metal tri-square for this machine only
* Needs thorough clean out – very mucky – WD40 then 3in1
* Make whole machine secure

**Spindle moulder**

* Metal polish for bed

**Table saw**

* Longer push sticks made from softwood not ply (500cm from handle)
* Sign on where to stand (not directly ahead of blade)
* Floor level isolator – on cable
* Spray for cleaning resin from blades
* Blade sharpening – SWEMCO?